Wireless communication requires additional hardware
on both EyeBot controller and PC (or workstation).
Also required is a software key that is entered
by pressing <I> / Reg .

--
Thomas Braunl, Apr. 2004
