# EyeNet - EyeBot Wireless Communication Network

We developed a wireless communication module, which plugs into the EyeBot controller and enables wireless communication utilising serial port no. 2. A number of EyeBots can communicate with each other without the need for a central host.

A second wireless module has been developed for a PC, which connects to the serial port (COM2) and the keyboard port (for power). This module will be linked into the network like any other EyeBot and can be used for remote controlling or monitoring robots.

#### Features

- Carrier frequency 433 MHz
- Transfer rate 9,600 Baud
- Fault-tolerant protocol
- Automatic network configuration
- New EyeBots will be automatically integrated
- Switched-off EyeBots will be automatically deleted