/*
* ramregs.s - define addresses of RAM registers in 68332
* adjust the setting of rammcr to reflect modmap bit
*/

rammcr  =     0xfffffb00      | ram module configuration register
ramtst  =     rammcr+2       | ram module test register
rambar  =     rammcr+4       | ram base address register
