EyeBot MK3 Features:
--------------------

Main Features:
- 25MHz 32bit Controller (Motorola 68332)
- 1MB RAM
- 512KB ROM (for system + user programs!)
- 1 parallel port
- 2 serial ports
- 8 digital inputs
- 8 digital outputs
- 8 analog inputs
- single compact PCB, almost same size as old EyeBot
- interface for color and grayscale camera
- large graphics LCD (128x64 pixels)
- 4 input buttons
- reset button, power switch
- speaker for audio output
- microphone for audio input
- battery level indication

Extensions to previous version:
- motor drivers for 2 DC motors included in board
- background debugger BDM circuit included in board
- "plug-and-play" connectors for motors, sensors, camera and serial port
  6 infrared sensors, 2 bumper sensors, 6 free analog inputs
- no special download cable required: 9pin RS232 extension cable
- wireless communication system integrated

Connectors for Actuators and Sensors:
- digital camera
- 2 DC motors with encoders
- 12 servos
- 6 infrared-sensors (or 6 free digital inputs)
- 2 bumpers (or 2 free digital inputs)
- 6 free analog inputs

Options:
- wireless communication modul

